CABLE ASSEMBLY

It’s a low noise cable(1.5 meters) for vibration measurement

It having 2 ends , one is TNC and another end is BNC .

BNC is connected to the instrument and TNC to the sensor

|  |  |
| --- | --- |
|  |  |

|  |  |
| --- | --- |
| https://pmequipments.com/assets/img/pm_equipments_logo.png | **PREDICTIVE MEASURING EQUIPMENTS**  Plot No 146, Phase 1, Mytrinagar, Madinaguda, Hyderabad – 500049  Mobile: +91-90593 40351, eMail: info@pmequipments.com, www.pmequipments.com |